**How to Boot Laptop for Imaging**

1. With the unimaged laptop, hook it up via ethernet to the server.
2. Mash F12 upon boot to get into the boot menu
3. Go into the bios setup
4. Look for “System Configuration” and expand the dropdown menu
5. Click on “Integrated NIC” and check “Enable UEFI Network Stack” if it isn’t already checked
6. Hit apply and then exit out of the BIOS screen
7. Upon reboot, keep hitting F12 until the one time boot menu shows up once again
8. Using the arrow keys, go down to “Onboard NIC(IPV4)” and hit enter
9. Follow the instructions on screen and configure how you would like